1. Plug your HUB (indoor) to power suppliers
2. Connect computer or your phone to **SNIFFER** network
3. Open web browser and access to address: **http://192.168.4.1**
4. Choose wifi network to connect then enter the password
5. Sniffer installed successfully.
6. Plug your SNIFFER (outdoor). Wait for data to display on HUB
7. Open <https://sniffer.axonactive.com/> to check data transferred from SNIFFER

**NOTE: If you want to reset Wi-Fi, click and hold for 2 seconds RESET button on HUB**