|  |
| --- |
| **INSTALLATION INSTRUCTIONS**  **1.** Plug your **SNIFFER** (outdoor) to power supplier  **2.** Connect computer or your phone to **SNIFFER** network  **3.** Open web browser and access to address: **http://192.168.4.1**  **4.** Choose Wifi network to connect then enter the password  **5.** Open <https://sniffer.axonactive.com/> to check  data transferred from SNIFFER  **NOTE: If you want to reset Wi-Fi, press RESET button (GREEN) on SNIFFER** |